# RMS Current Measurements

After acquiring values from CTs the function calculates RMS values for 3 Phases. These values are for indication. The protection function measurements are not modelled in this example.